|  |  |  |
| --- | --- | --- |
| A9010 | Instrument cluster | 2 |
| A9020 | Flasher unit | 44 |
| A9030 | L-Jetronic control unit | 79 |
| A9040 | ABS control unit | 86 |
| A9050 | Ignition control unit | 58 |
| B9000 | Fuel gauge | 12 |
| B9010 | Inductive transmitter | 11 |
| B9020 | Temperature transmitter | 71 |
| B9030 | ABS front sensor | 72 |
| B9031 | ABS rear sensor | 74 |
| B9040 | Airflow meter | 84 |
| B9050 | Magnetic gate | 57 |
| E9000 | Headlight | 20 |
| E9001 | Low-beam headlight | 20 |
| E9002 | High-beam headlight | 20 |
| E9010 | Headlight | 76 |
| E9020 | Parking light | 24 |
| E9030 | Instrument lighting | 2 |
| G9000 | Battery | 66 |
| G9010 | Alternator | 63 |
| H9000 | Battery charge warning light | 4 |
| H9010 | Oil pressure warning light | 5 |
| H9030 | Front left flashing turn indicator | 5 |
| H9041 | Turn indicator repeater, right | 5 |
| H9042 | Turn indicator repeater, left | 5 |
| H9050 | Brake light | 4 |
| H9060 | Neutral telltale | 3 |
| H9070 | Choke telltale | 3 |
| H9080 | Fuel level telltale | 2 |
| H9090 | Bulb telltale | 4 |
| H91 00 | ### ABS-Kontrolleuchte ### | 4 |
| H9110 | Gear indicator | 3 |
| H9200 | Brake light | 76 |
| H9500 | Front left flashing turn indicator | 5 |
| H9510 | Front right flashing turn indicator | 3 |
| H9520 | Rear left flashing turn indicator | 83 |
| H9530 | Rear right flashing turn indicator | 83 |
| H9921 | Twin-tone horn, left | 2 |
| H9922 | Twin-tone horn, right | 2 |
| K9000 | Starter motor relay | 54 |
| K9010 | Load relief relay | 43 |
| K9020 | Flasher unit | 46 |
| K9030 | Horn relay | 49 |
| K9040 | Injection Relay | 45 |
| K9050 | Bulb monitoring unit | 58 |
| K9060 | ABS warning relay | 77 |
| K9070 | ABS relay | 77 |
| M9000 | Starter motor | 66 |
| M9010 | ### Kraftstoffpumpe ### | 12 |
| M9020 | ### Lüftermotor ### | 22 |
| N9000 | Thermostat | 55 |
| P9000 | Speedometer | 2 |
| P9010 | Revolution counter | 2 |
| R9001 | ### Zündkerze 1 ### | 62 |
| R9002 | ### Zündkerze 2 ### | 67 |
| R9003 | ### Zündkerze 3 ### | 65 |
| R9004 | ### Zündkerze 4 ### | 61 |
| S9000 | Ignition switch | 23 |
| S9100 | Combined switch, left | 24 |
| S9110 | High-beam headlight | 21 |
| S9121 | Turn indicator switch, left | 21 |
| S9130 | Horn switch | 21 |
| S9200 | Combined switch, right | 29 |
| S9210 | ### Lichtschalter ### | 30 |
| S9220 | Turn indicator switch, right | 31 |
| S9230 | Kill switch | 32 |
| S9235 | Turn indicator cancel switch | 34 |
| S9240 | Starter switch | 33 |
| S9300 | Brake light switch, hand-operated | 39 |
| S9310 | Brake light switch, foot-operated | 63 |
| S9400 | Oil pressure switch | 11 |
| S9410 | Choke switch with telltale lamp | 14 |
| S9420 | Transmission switch | 20 |
| S9430 | Clutch switch | 41 |
| S9440 | Hazard warning flasher switch | 45 |
| S9450 | Throttle butterfly switch | 84 |
| S9460 | ABS button | 70 |
| T9010 | Ignition coil 1 | 61 |
| T9020 | Ignition coil 2 | 66 |
| V9000 | Clock | 3 |
| X9000 | Plug connection - engine wiring harness | 72 |
| X9020 | Plug connection - rear section | 73 |
| X9030 | Plug connection - fairing | 10 |
| X9040 | Plug connection - oil pressure gauge | 12 |
| X9050 | Plug connection - special equipment | 50 |
| X9060 | Plug connection - alarm system | 56 |
| X9070 | Plug connection - ABS diagnosis | 86 |
| X9080 | Plug connection - heated handlebar grips | 22 |
| X9100 | Plug connection - auxiliary instruments | 25 |
| Y9001 | Valve 1 | 84 |
| Y9002 | Valve 2 | 84 |
| Y9003 | Valve 3 | 84 |
| Y9004 | ### Ventil 4 ### | 84 |
| Y9010 | ABS pressure modulator, front | 78 |
| Y9020 | ABS pressure modulator, rear | 78 |